# Supported Devices

## USB/Serial Bridge Chips

Serial contains built-in drivers for all devices based on the USB/Serial bridge chips listed below:

Manufacturer | Device Family
--- | ---
FTDI | FT232x, FT230X, FT231X, FT234X, FT2232H, FT4232H, FT260 (HID)
Prolific | PL2303, PL2303G Series
WCH (Jiangsu Qin Heng) | CH340, CH341 Series
Silicon Labs | CP210x Series, CP2110 (HID)
Moschip | MCS78x0 Series
MCT | MCTU232
Texas Instruments | TUSB3410
Microchip | MCP2200, MCP2221 (CDC)
Cypress Semiconductor | CY7C6521x Series (CDC)

## Other Devices

Serial also contains built-in drivers for the following devices:

Manufacturer | Device
--- | ---
All | Any device that implements the Communications Device Class (CDC) interface
Keyspan / Tripp-Lite | USA-18X, USA-19, USA-19Qi, USA-19QW, USA-28, USA-28X, USA-28XA, USA-28XB, USA-49W, USA-49WLC, USA-49WG, USA-49WGv2 (i.e. USA-49WR)
Moxa | Uport 11xx

Serial supports any other serial device that macOS supports via DriverKit (macOS 10.15+) or a kernel extension.